**COMMERCIAL SYSTEM**

**WEIGHT**: 170 lbs

**HEIGHT**: 35 inches

**WIDTH**: 45 inches

**LENGTH**: 62 inches

**MATERIALS USED**: Ide frames and Steps are built from 1.0 x 1.0 x .100 and 2.0 x 3.0 x .10 ASTM A500 Grade B and A36/44W material. Bars are 1.0 dia. C1018 and 1.0 x .125 wall ASTM A513 Type 1 Tube. Step tops are built with 5/8 Plywood, EVA BCW-25 Foam and Vinyl (polyvinyl chloride Good for up to -40 Degrees C). Loops for attaching Bands are ¼ dia. C1018

**HOW MUCH WEIGHT IT CAN HOLD?** Due to the CoreStrength1’s excellent durability, we have had several 300lb+ athletes working out on the machine simultaneously.

**GUARANTEE**: The CoreStrength1 is guaranteed 100% for 2 years against any factory defect.